**Příloha č. 1 veřejné zakázky**

**Zajištění SW a HW podpory výrobce Oracle na 12 měsíců pro VoZP ČR**

1. **Popis stávajícího stavu**

Předmětem této veřejné zakázky je dodání SW a HW podpory výrobce Oracle na 12 měsíců dle specifikace uvedené v bodu č. 2 této přílohy.

Tato HW a SW podpora slouží k zajištění bezporuchového běhu Integrovaného informačního systému VoZP ČR.

1. **Požadavky na dodávku – specifikace HW a SW podpory**

Položka: 5547767 SW

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Start Date | Item Name | End Date | CSI Number | Asset Party Owner Number | No of Users | License Type |
| 01-FEB-2016 | Oracle Database Standard Edition - Processor Perpetual | 31-JAN-2017 | 18601112 | 57556416 | 4 | FULL USE |
| 01-FEB-2016 | Oracle WebLogic Suite - Processor Perpetual | 31-JAN-2017 | 18601112 | 57556416 | 6 | FULL USE |
| 01-FEB-2016 | Oracle SOA Suite for Oracle Middleware - Processor Perpetual | 31-JAN-2017 | 18601112 | 57556416 | 6 | FULL USE |
| 01-FEB-2016 | Oracle Business Intelligence Suite Enterprise Edition Plus - Named User Plus Perpetual | 31-JAN-2017 | 18601112 | 57556416 | 50 | FULL USE |
| 01-FEB-2016 | Oracle Business Intelligence Publisher - Processor Perpetual | 31-JAN-2017 | 18601112 | 57556416 | 1 | FULL USE |

Položka: 5532908 HW

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Start Date | Item Name | End Date | CSI Number | Quantity |
| 01-FEB-2016 | Sun Fire X4270 M2 server | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Sun Fire X4270 M2 server | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Sun Fire X4270 M2 server: base 2.5-inch chassis with motherboard, one 1,200 W AC PSU,  and service processor (for factory installation) | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Rack mount slide rail kit tooled (for factory installation) | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Sun x4 Quad-port Gigabit Ethernet Adapter UTP | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | One 300 GB 10000 rpm 2.5-inch SAS-2 HDD with bracket (for factory installation) | 31-JAN-2017 | 18568680 | 8 |
| 01-FEB-2016 | 1 Intel(R) Xeon(R) X5690 6-core 3.46 GHz processor (for factory installation) | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | Power cord: Sun Rack 2 jumper, 2 meters, C14RA plug, C13 connector, 13 A (for factory installation) | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | Cable management arm (for factory installation) | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | One 8 GB DDR3-1333 registered low-voltage DIMM (for factory installation) | 31-JAN-2017 | 18568680 | 9 |
| 01-FEB-2016 | 1,200 W AC PSU (for factory installation) | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Sun Storage 6 Gb SAS PCIe RAID HBA, Internal: 8 port and 512 MB cache (for factory installation) | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | StorageTek 8 Gb Fibre Channel PCIe HBA dual port QLogic (for factory Installation) | 31-JAN-2017 | 18568680 | 2 |

Položka: 5531615 HW

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Start Date | Item Name | End Date | CSI Number | Quantity |
| 01-FEB-2016 | Jumper Cable Kit: 1 x 2m C13 | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | Sun Server X2-8 for non-EU countries: model family | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Sun Fire X4800 M2 server: model family | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Two 4 GB DDR3-1066 DIMMs (for factory installation) | 31-JAN-2017 | 18568680 | 16 |
| 01-FEB-2016 | One 600 GB 10000 rpm 2.5-inch SAS-2 HDD with bracket (for factory installation) | 31-JAN-2017 | 18568680 | 6 |
| 01-FEB-2016 | Sun Server X2-8: Network Express Module with four 10 GbE SFP+ ports, two x4 SAS 2.0 mini-ports, 4 GbE pass-through interfaces for non-EU countries (for factory installation) | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | Power cord: Sun Rack 2 jumper, 2 meters, C14RA plug, C13 connector, 13 A (for factory installation) | 31-JAN-2017 | 18568680 | 4 |
| 01-FEB-2016 | Sun Server X2-8 for non-EU countries: base chassis | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Sun x4 PCIe QGE ExpressModule | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | 1 Intel(R) Xeon(R) E7-8870 10-core 2.4 GHz processor with heat sink (for factory installation) | 31-JAN-2017 | 18568680 | 4 |
| 01-FEB-2016 | CPU module with 32 DIMM slots and 2 USB ports for non-EU countries | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | 6Gb/s SAS REM RAID HBA, ATO | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Sun Server X2-8 for non-EU countries: model family | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Sun Fire X4800 M2 server: model family | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Two 4 GB DDR3-1066 DIMMs (for factory installation) | 31-JAN-2017 | 18568680 | 16 |
| 01-FEB-2016 | One 600 GB 10000 rpm 2.5-inch SAS-2 HDD with bracket (for factory installation) | 31-JAN-2017 | 18568680 | 6 |
| 01-FEB-2016 | Sun Server X2-8: Network Express Module with four 10 GbE SFP+ ports, two x4 SAS 2.0 mini-ports, 4 GbE pass-through interfaces for non-EU countries (for factory installation) | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | Power cord: Sun Rack 2 jumper, 2 meters, C14RA plug, C13 connector, 13 A (for factory installation) | 31-JAN-2017 | 18568680 | 4 |
| 01-FEB-2016 | Sun Server X2-8 for non-EU countries: base chassis | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Sun x4 PCIe QGE ExpressModule | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | 1 Intel(R) Xeon(R) E7-8870 10-core 2.4 GHz processor with heat sink (for factory installation) | 31-JAN-2017 | 18568680 | 4 |
| 01-FEB-2016 | CPU module with 32 DIMM slots and 2 USB ports for non-EU countries | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | 6Gb/s SAS REM RAID HBA, ATO | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Brocade rack rail kit, supports 16.90 inches switches | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | Brocade 300 Switch with eight 8 Gb activated ports and E\_port license | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | BROCADE 300 24-PORT FC 8G SFP | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Brocade 300 Switch with eight 8 Gb activated ports and E\_port license | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | BROCADE 300 24-PORT FC 8G SFP | 31-JAN-2017 | 18568680 | 1 |

Položka: 5530225 HW

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Start Date | Item Name | End Date | CSI Number | Quantity |
| 01-FEB-2016 | Sun Fire X4270 M2 server | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Sun Fire X4270 M2 server | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | One 300 GB 10000 rpm 2.5-inch SAS-2 HDD with bracket (for factory installation) | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | One 8 GB DDR3-1333 registered low-voltage DIMM (for factory installation) | 31-JAN-2017 | 18568680 | 9 |
| 01-FEB-2016 | Cable management arm (for factory installation) | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Sun Storage 6 Gb SAS PCIe RAID HBA, Internal: 8 port and 512 MB cache (for factory installation) | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Sun Dual 10GbE SFP+ PCIe Low Profile Adapter | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | 1 Intel(R) Xeon(R) X5690 6-core 3.46 GHz processor (for factory installation) | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | 1,200 W AC PSU (for factory installation) | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Power cord: Sun Rack 2 jumper, 2 meters, C14RA plug, C13 connector, 13 A (for factory installation) | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | StorageTek 8 Gb Fibre Channel PCIe HBA dual port QLogic (for factory Installation) | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | Sun 10Gbps Dual Rate SFP+ SR | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | Sun x4 Quad-port Gigabit Ethernet Adapter UTP | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Rack mount slide rail kit tooled (for factory installation) | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Sun Fire X4270 M2 server: base 2.5-inch chassis with motherboard, one 1,200 W AC PSU,  and service processor (for factory installation) | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Sun Fire X4270 M2 server | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Sun Fire X4270 M2 server | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | One 300 GB 10000 rpm 2.5-inch SAS-2 HDD with bracket (for factory installation) | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | One 8 GB DDR3-1333 registered low-voltage DIMM (for factory installation) | 31-JAN-2017 | 18568680 | 9 |
| 01-FEB-2016 | Cable management arm (for factory installation) | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Sun Storage 6 Gb SAS PCIe RAID HBA, Internal: 8 port and 512 MB cache (for factory installation) | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Sun Dual 10GbE SFP+ PCIe Low Profile Adapter | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | 1 Intel(R) Xeon(R) X5690 6-core 3.46 GHz processor (for factory installation) | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | 1,200 W AC PSU (for factory installation) | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Power cord: Sun Rack 2 jumper, 2 meters, C14RA plug, C13 connector, 13 A (for factory installation) | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | StorageTek 8 Gb Fibre Channel PCIe HBA dual port QLogic (for factory Installation) | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | Sun 10Gbps Dual Rate SFP+ SR | 31-JAN-2017 | 18568680 | 2 |
| 01-FEB-2016 | Sun x4 Quad-port Gigabit Ethernet Adapter UTP | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Rack mount slide rail kit tooled (for factory installation) | 31-JAN-2017 | 18568680 | 1 |
| 01-FEB-2016 | Sun Fire X4270 M2 server: base 2.5-inch chassis with motherboard, one 1,200 W AC PSU,  and service processor (for factory installation) | 31-JAN-2017 | 18568680 | 1 |

1. **Rozpočet**

Uchazeč zpracuje rozpočet do níže uvedené tabulky tak, že uvede cenu jednotlivých položek bez DPH, DPH položky a cenu položky včetně DPH. Do dalších tabulek uvede cenu za jednotlivé součásti položky bez DPH. Tabulka Rozpočet bude přílohou Smlouvy.

|  |  |  |  |
| --- | --- | --- | --- |
| **položka** | **Cena v Kč bez DPH** | **DPH** | **Cena v Kč včetně DPH** |
| 5547767 SW |  |  |  |
| 5532908 HW |  |  |  |
| 5531615 HW |  |  |  |
| 5530225 HW |  |  |  |
| **celkem** |  |  |  |

Položka: 5547767 SW

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Start Date | Item Name | End Date | CSI Number | Asset Party Owner Number | No of Users | License Type | Cena v Kč bez DPH |
| 01-FEB-2016 | Oracle Database Standard Edition - Processor Perpetual | 31-JAN-2017 | 18601112 | 57556416 | 4 | FULL USE |  |
| 01-FEB-2016 | Oracle WebLogic Suite - Processor Perpetual | 31-JAN-2017 | 18601112 | 57556416 | 6 | FULL USE |  |
| 01-FEB-2016 | Oracle SOA Suite for Oracle Middleware - Processor Perpetual | 31-JAN-2017 | 18601112 | 57556416 | 6 | FULL USE |  |
| 01-FEB-2016 | Oracle Business Intelligence Suite Enterprise Edition Plus - Named User Plus Perpetual | 31-JAN-2017 | 18601112 | 57556416 | 50 | FULL USE |  |
| 01-FEB-2016 | Oracle Business Intelligence Publisher - Processor Perpetual | 31-JAN-2017 | 18601112 | 57556416 | 1 | FULL USE |  |

Položka: 5532908 HW

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Start Date | Item Name | End Date | CSI Number | Quantity | Cena v Kč bez DPH |
| 01-FEB-2016 | Sun Fire X4270 M2 server | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Sun Fire X4270 M2 server | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Sun Fire X4270 M2 server: base 2.5-inch chassis with motherboard, one 1,200 W AC PSU,  and service processor (for factory installation) | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Rack mount slide rail kit tooled (for factory installation) | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Sun x4 Quad-port Gigabit Ethernet Adapter UTP | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | One 300 GB 10000 rpm 2.5-inch SAS-2 HDD with bracket (for factory installation) | 31-JAN-2017 | 18568680 | 8 |  |
| 01-FEB-2016 | 1 Intel(R) Xeon(R) X5690 6-core 3.46 GHz processor (for factory installation) | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | Power cord: Sun Rack 2 jumper, 2 meters, C14RA plug, C13 connector, 13 A (for factory installation) | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | Cable management arm (for factory installation) | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | One 8 GB DDR3-1333 registered low-voltage DIMM (for factory installation) | 31-JAN-2017 | 18568680 | 9 |  |
| 01-FEB-2016 | 1,200 W AC PSU (for factory installation) | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Sun Storage 6 Gb SAS PCIe RAID HBA, Internal: 8 port and 512 MB cache (for factory installation) | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | StorageTek 8 Gb Fibre Channel PCIe HBA dual port QLogic (for factory Installation) | 31-JAN-2017 | 18568680 | 2 |  |

Položka: 5531615 HW

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Start Date | Item Name | End Date | CSI Number | Quantity | Cena v Kč bez DPH |
| 01-FEB-2016 | Jumper Cable Kit: 1 x 2m C13 | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | Sun Server X2-8 for non-EU countries: model family | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Sun Fire X4800 M2 server: model family | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Two 4 GB DDR3-1066 DIMMs (for factory installation) | 31-JAN-2017 | 18568680 | 16 |  |
| 01-FEB-2016 | One 600 GB 10000 rpm 2.5-inch SAS-2 HDD with bracket (for factory installation) | 31-JAN-2017 | 18568680 | 6 |  |
| 01-FEB-2016 | Sun Server X2-8: Network Express Module with four 10 GbE SFP+ ports, two x4 SAS 2.0 mini-ports, 4 GbE pass-through interfaces for non-EU countries (for factory installation) | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | Power cord: Sun Rack 2 jumper, 2 meters, C14RA plug, C13 connector, 13 A (for factory installation) | 31-JAN-2017 | 18568680 | 4 |  |
| 01-FEB-2016 | Sun Server X2-8 for non-EU countries: base chassis | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Sun x4 PCIe QGE ExpressModule | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | 1 Intel(R) Xeon(R) E7-8870 10-core 2.4 GHz processor with heat sink (for factory installation) | 31-JAN-2017 | 18568680 | 4 |  |
| 01-FEB-2016 | CPU module with 32 DIMM slots and 2 USB ports for non-EU countries | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | 6Gb/s SAS REM RAID HBA, ATO | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Sun Server X2-8 for non-EU countries: model family | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Sun Fire X4800 M2 server: model family | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Two 4 GB DDR3-1066 DIMMs (for factory installation) | 31-JAN-2017 | 18568680 | 16 |  |
| 01-FEB-2016 | One 600 GB 10000 rpm 2.5-inch SAS-2 HDD with bracket (for factory installation) | 31-JAN-2017 | 18568680 | 6 |  |
| 01-FEB-2016 | Sun Server X2-8: Network Express Module with four 10 GbE SFP+ ports, two x4 SAS 2.0 mini-ports, 4 GbE pass-through interfaces for non-EU countries (for factory installation) | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | Power cord: Sun Rack 2 jumper, 2 meters, C14RA plug, C13 connector, 13 A (for factory installation) | 31-JAN-2017 | 18568680 | 4 |  |
| 01-FEB-2016 | Sun Server X2-8 for non-EU countries: base chassis | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Sun x4 PCIe QGE ExpressModule | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | 1 Intel(R) Xeon(R) E7-8870 10-core 2.4 GHz processor with heat sink (for factory installation) | 31-JAN-2017 | 18568680 | 4 |  |
| 01-FEB-2016 | CPU module with 32 DIMM slots and 2 USB ports for non-EU countries | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | 6Gb/s SAS REM RAID HBA, ATO | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Brocade rack rail kit, supports 16.90 inches switches | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | Brocade 300 Switch with eight 8 Gb activated ports and E\_port license | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | BROCADE 300 24-PORT FC 8G SFP | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Brocade 300 Switch with eight 8 Gb activated ports and E\_port license | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | BROCADE 300 24-PORT FC 8G SFP | 31-JAN-2017 | 18568680 | 1 |  |

Položka: 5530225 HW

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Start Date | Item Name | End Date | CSI Number | Quantity | Cena v Kč bez DPH |
| 01-FEB-2016 | Sun Fire X4270 M2 server | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Sun Fire X4270 M2 server | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | One 300 GB 10000 rpm 2.5-inch SAS-2 HDD with bracket (for factory installation) | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | One 8 GB DDR3-1333 registered low-voltage DIMM (for factory installation) | 31-JAN-2017 | 18568680 | 9 |  |
| 01-FEB-2016 | Cable management arm (for factory installation) | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Sun Storage 6 Gb SAS PCIe RAID HBA, Internal: 8 port and 512 MB cache (for factory installation) | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Sun Dual 10GbE SFP+ PCIe Low Profile Adapter | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | 1 Intel(R) Xeon(R) X5690 6-core 3.46 GHz processor (for factory installation) | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | 1,200 W AC PSU (for factory installation) | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Power cord: Sun Rack 2 jumper, 2 meters, C14RA plug, C13 connector, 13 A (for factory installation) | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | StorageTek 8 Gb Fibre Channel PCIe HBA dual port QLogic (for factory Installation) | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | Sun 10Gbps Dual Rate SFP+ SR | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | Sun x4 Quad-port Gigabit Ethernet Adapter UTP | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Rack mount slide rail kit tooled (for factory installation) | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Sun Fire X4270 M2 server: base 2.5-inch chassis with motherboard, one 1,200 W AC PSU,  and service processor (for factory installation) | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Sun Fire X4270 M2 server | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Sun Fire X4270 M2 server | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | One 300 GB 10000 rpm 2.5-inch SAS-2 HDD with bracket (for factory installation) | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | One 8 GB DDR3-1333 registered low-voltage DIMM (for factory installation) | 31-JAN-2017 | 18568680 | 9 |  |
| 01-FEB-2016 | Cable management arm (for factory installation) | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Sun Storage 6 Gb SAS PCIe RAID HBA, Internal: 8 port and 512 MB cache (for factory installation) | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Sun Dual 10GbE SFP+ PCIe Low Profile Adapter | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | 1 Intel(R) Xeon(R) X5690 6-core 3.46 GHz processor (for factory installation) | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | 1,200 W AC PSU (for factory installation) | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Power cord: Sun Rack 2 jumper, 2 meters, C14RA plug, C13 connector, 13 A (for factory installation) | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | StorageTek 8 Gb Fibre Channel PCIe HBA dual port QLogic (for factory Installation) | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | Sun 10Gbps Dual Rate SFP+ SR | 31-JAN-2017 | 18568680 | 2 |  |
| 01-FEB-2016 | Sun x4 Quad-port Gigabit Ethernet Adapter UTP | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Rack mount slide rail kit tooled (for factory installation) | 31-JAN-2017 | 18568680 | 1 |  |
| 01-FEB-2016 | Sun Fire X4270 M2 server: base 2.5-inch chassis with motherboard, one 1,200 W AC PSU,  and service processor (for factory installation) | 31-JAN-2017 | 18568680 | 1 |  |

Praha dne: ……………… dne

…………………………………. ………………………………….

objednatel poskytovatel